; bcmusb.INF
; Install information file for BeceemNDIS Driver
; Copyright (c) 2006 Beceem Communications Pvt. Ltd.
;
; File created on 6/30/2005
;
;--------- Version Section ---------------------------------------------------

[version]
signature="$CHICAGO$"
Class=Net
ClassGUID = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%Mfg%
Compatible  = 1
DriverVer=08/27/2009, 5.2.115.0
; Millenium exclusive suffix
MillenniumPreferred = .me
CatalogFile = drxvi314.cat

[Manufacturer]
%Mfg%=Models

[ControlFlags]
;Note: Uncomment next line if your NIC is not to be installed manually
;ExcludeFromSelect = USB\VID_198F&PID_0300

[Models]
; Note 1. Optionally, add more NIC models supported by this file
;
; DisplayName        Section           hw-id
; -----------        -------           ------

%*bcm.devicedesc%=*bcm.ndi, BCMBus\BcmWiMAX 

;-------------------------------------------------------------
; Win2K
[*bcm.ndi.NT]
AddReg = bcm.w2k.reg, bcm.params.reg
CopyFiles = bcm.w2k.CopyFiles
;
Characteristics = 0x81 ; NCF_ flags
    ;Characteristics = 0x84			; NCF_HAS_UI & NCF_PHYSICAL
    ;BusType	        = 1			; ISA


;-------------------------------------------------------------
; Win2K
[*bcm.ndi.NT.Services]
AddService = bcm, 2, bcm.Service, bcm.EventLog

;-------------------------------------------------------------
; Win2K
[bcm.w2k.reg]
HKR, Ndi, Service, 0,"bcm"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"


[bcm.w2k.CopyFiles]
drxvi314.sys
macxvi200.bin
macxvi.cfg

;-----------------------------------------------------------
; Sources
[SourceDisksNames]
99=%bcm_disk%,"",0

[SourceDisksFiles]
drxvi314.sys = 99
macxvi200.bin = 99
macxvi.cfg = 99

;-----------------------------------------------------------
; Destination Dir
[DestinationDirs]
DefaultDestDir            =11 ; system dir
bcm.w2k.CopyFiles    =12 ; W2K: system32\drivers

;-------------------------------------------------------------------------------
; Optional Custom Parameters in the Registry ("Advanced" menu).
[bcm.params.reg]


HKR, NDI\params\MTU, ParamDesc, 0, %MTU%
HKR, NDI\params\MTU, type , 0, REG_DWORD
HKR, NDI\params\MTU, default,0, "1400"
HKR, NDI\params\MTU, min, 0, "1300"
HKR, NDI\params\MTU, max, 0, "1500"


;------------------------------------------------------------
; W2K Service entry, log, etc.
[bcm.Service]
DisplayName     = %bcm.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\drxvi314.sys
LoadOrderGroup  = NDIS

[bcm.EventLog]
AddReg = bcm.AddEventLog.reg

[bcm.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7


;-------------------------------------------------------------------------------
; Localizable Strings
;
[strings]
Mfg                                       = "Beceem Communications Pvt. Ltd"
*bcm.DeviceDesc         = "WiMAX Network Adapter"
bcm.devicedesc          = "WiMAX Network Adapter"
bcm.Service.DispName    = "WiMAX Network Adapter"
Mode          	        = "Sample Parameter"
Mode_basic  	        = "Basic"
Mode_cool 	        = "Cool"
bcm_disk    	        = "WiMAX Device Driver Install Disk"
Disabled      	        = "Disabled"
Enabled      	        = "Enabled"

MTU			= "MTU"
